* As technology improving, there are more and more application of mobile robots in different fields, such as in factories, logistics and hospitals. One of the biggest advantages of mobile robots is the ability to transport items and move automatically without direct human control. This not only saves on labor costs but also reduces so much tedious work that people have to do. Because of this, improving the autonomy of mobile robots can greatly expand their use, allowing more people to benefit from their capabilities. So, to achieve this, I focus on Motion planning for mobile robots, which plays a crucial role in enabling their autonomy.
* What is Motion planning in the field of robotics? Typically, it finds a continuous sequence of valid configurations that safely and efficiently guide a robot from start to goal. There are two critical parts: global planning and local planning. My research mainly focuses on local planning, but I need to introduce both first.

Global planning is like navigation in Google Maps; it creates a clear route from the starting point to the goal, telling robots how to avoid static obstacles. On the other hand, local planning must handle all emergencies in real time. It generates a motion command in every short time period that helps robots evade dynamic objects, just like a driver constantly making decisions on the go. Therefore, a better local planning system should help mobile robots navigate highly dynamic and complex environments, consequently improving their autonomy.

* There are several methods for solving local planning problems. Artificial Potential Fields (APF) model obstacles as repulsive forces and goals as attractive forces, allowing mobile robots to avoid obstacles in real-time. However, they often struggle with local minima issues.

Dynamic Window Approach (DWA) samples velocity commands within dynamic constraints and scores them based on clearance, velocity, and heading. While effective, it struggles with continuously moving obstacles. In fact, one of our former lab members focused on addressing this issue.

Velocity Obstacles (VO) predict collision regions in velocity space and select safe velocities. This method is highly effective for multi-agent systems but requires accurate motion prediction of surrounding obstacles.

Model Predictive Control (MPC) optimizes trajectories over a short horizon while respecting dynamic constraints. It effectively handles robot dynamics and obstacles but can become computationally expensive as the planning horizon increases.